|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **1. GENERAL DATA** | | | | | | | |
| PROJECT NAME: | | | PROJECT NO.: | | | | |
| WC P.O. / CONTRACT NO.: | | | LINE / ITEM NO.: | | | | |
|  | | |  | | | | |
| **2. DATA LOGGER DATA** | | | | | | | |
| WC TAG NO.: | | | | WC DESCRIPTION: | | | |
| WC DWG NO.: | | | | MANUFACTURER: | | | |
| MODEL NO.: | | | | SERIAL NO.: | | | |
| MODEM TYPE (e.g. 4G): | | | | POWER: | | | |
|  | | | |  | | | |
| **3. TEST** | | **DONE**  **/YES** | | | **NO** | **N/A** | **COMMENTS/DETAILS** |
| 1 | Confirm data logger can be connected to in the relevant software |  | | |  |  |  |
| 2 | Confirm data logger has been loaded with the most recent firmware available in MDT |  | | |  |  |  |
| 3 | Confirm data logger has been loaded with the correct configuration |  | | |  |  |  |
| 4 | Confirm data logger has sufficient signal strength |  | | |  |  |  |
| 5 | Confirm data logger is able to poll and upload data |  | | |  |  |  |
| 6 | Confirm battery voltage or power supply voltage is healthy |  | | |  |  |  |
| 7 | Confirm unsolicited poll (manually activated by magnetic reed switch) has been configured |  | | |  |  |  |

|  |
| --- |
| **4. REMARKS / REMEDIAL ACTIONS** |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **5. SIGNOFFS** | |  | | |
| NAME (PRINT) | COMPANY / ROLE | | SIGNATURE | DATE |
| NAME (PRINT) | COMPANY / ROLE | | SIGNATURE | DATE |
| NAME (PRINT) | COMPANY / ROLE | | SIGNATURE | DATE |