**Referenced to Water Corporation Standards: DS21, DS22, DS26-02, DS26-13, DS26-16, DS26-28, and DS26-29.**

|  |  |
| --- | --- |
| **1. GENERAL DATA** | |
| PROJECT NAME: | PROJECT NO: |
| IDENTIFICATION: |  |

|  |  |
| --- | --- |
| **2. TRANSFORMER DATA** | |
| TYPE: OIL FILLED  DRY | |
| SITE REQUIREMENT: INDOOR  OUTDOOR  KIOSK | |
| MOUNTING: GROUND  POLE | |
| MAKE: | SERIAL NO: |
| ENCLOSURE PROTECTION: | COOLING: |
| INSULATION CLASS: | VECTOR GROUP: |
| KVA RATING: | FREQUENCY: |
| PRIMARY VOLTAGE: | PRIMARY CURRENT: |
| SECONDARY VOLTAGE: | SECONDARY CURRENT: |
| TERTIARY VOLTAGE: | TERTIARY CURRENT: |
| MF DWG NO.(S): | WC TRANSFORMER NO.: |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **3. INSPECTION** | | **DONE**  **/YES** | **NO** | **N/A** | **COMMENTS/DETAILS** |
| 1 | Location of transformer. |  | | | |
| 2 | Transformer undamaged. |  |  |  |  |
| 3 | Transformer orientated as per drawings. |  |  |  |  |
| 4 | Identification and danger labels fitted. |  |  |  |  |
| 5 | Door and cable box interlocks operate correctly. |  |  |  |  |
| 6 | HV cables installed correctly. |  |  |  |  |
| 7 | LV cables installed correctly. |  |  |  |  |
| 8 | Over temperature/over pressure control cables installed correctly. |  |  |  |  |
| 9 | Surge diverters installed correctly. |  |  |  |  |
| 10 | Earth Fault CT installed correctly. |  |  |  |  |
| 11 | Earthing cables installed correctly. |  |  |  |  |

|  |
| --- |
| **4. REMARKS / REMEDIAL ACTIONS** |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **5. SIGNOFFS** | |  | | |
| NAME (PRINT) | COMPANY / ROLE | | SIGNATURE | DATE |
| NAME (PRINT) | COMPANY / ROLE | | SIGNATURE | DATE |
| NAME (PRINT) | COMPANY / ROLE | | SIGNATURE | DATE |