{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Ex Register"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":4,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ex Register","index":0,"n_rows":4,"n_cols":18,"rows_kept":4,"cut":false,"hidden":false,"merged":[[1,17,2,17],[1,14,2,14],[1,15,2,15],[1,16,2,16],[1,5,2,5],[1,9,2,9],[1,13,2,13],[1,12,2,12],[1,11,2,11],[1,7,2,7],[1,8,2,8],[1,1,2,1],[1,6,2,6],[1,3,2,3],[1,10,2,10],[1,0,2,0],[1,2,2,2],[1,4,2,4]]}
["Ex Register for <<  SITE NAME  >>"]
["No.","Equipment No./ID","Equipment Description","Equipment Make","Equipment Model","Certificate Number","Zone","Gas Group","Temp Class","Protection - Gas Group - Temp Class","Location","P&IDs","Datasheet","Loop Drawing","ISB Model \n(if applicable)","ISB Cert No \n(if applicable)","ISB Loop Calc No\n(if applicable)","Comment"]
[]
[0,"LSH22081","Ultrasonic Level Switch","Siemens","Pointek ULS200","Aus Ex 3702 X",2,"2A","T1","Ex ds IIC T6","Inlet Screening","JS25-60-22-2","JS25-DS223","JS25-42-430.1",null,null,null,"As an example only"]